Meter Installation Procedure
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1. Site Preparation
2. Installation Procedure
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Installation Procedure
a) Disconnection of the old Meter (ELSTER)
Taking meter Readings
Identify the cable
Disconnection from all power sources of supply
Dis-mounting the old Meter
Power sources:
Current source
Voltage source
Auxiliary supply
b) Installation of the new Meter (Landis + GYR E650)
Mounting of the New Meter
Re-connecting the Current, VT and Auxiliary Cables
Powering of the Meter for Configuration
c) Configuration
CT Ratio
VT Ratio
Date & Time
d) Local Commissioning
e) Final Commissioning




